**Hardware requirements for Rover distributed comms**

(Quantities for implementation prototype - adjust depending on number of nodes)

Linkit x4 (NanoPi Neo?) + SD cards w/ Linux

Ethernet switch (min. 5 ports)

Ethernet cables (min. x5)